2019.08.27 (V1.0.8)
	Fix bug with FocusMax.
	Fix bug with SGPro.
	The debug message sent to Ascom prints the value of the received "M" command.

30 September 2018 (V2.0.4)
	Modification due to MFOC ASCOM v1.6.0.

31 August 2017 (v1.0.3)
	The value of "TempComp" can be set from +-5000.	
	Some bug fixes.
	Log in English
	After the firmware is loaded, it is necessary to start the Factory Reset function!

01 March 2017 (v1.0.2)
	The value of "TempComp" can be set from +-255.
	The value of "BacklChg" can be set from 0 to 255.
	The value of "Offsets" can be set from +-100.
	Eliminated the "Temp Track" menu.
	The "TempComp" and "TempTrackDir" set to "Focuser" menu.
	Other bug fixes.

12 December 2016 (V1.0.1)
	Troubleshooting the motor direction change. Now it does not require a reboot of the CW/CCW switched.
	Troubleshooting settings via Ascom connection.		
	Maximum position up to 65535!
	
18 August 2016 (V1.0.0)
	First version!
	 

